               MMA CORRELATOR BLOCK DIAGRAM

                125 MHz ECL DATA

1

15

40
1

34
                                                                                         DELAYED MEMORY

                                                                                         32K X 128 RAM

                                                      SWITCHING
                                                       MATRIX

                   32 X 2

                                 DELAY
                                 LINES

4 GHz SAMPLER

4 GHz SAMPLER

4 GHz SAMPLER

                   32 X 2

                   32 X 2

                                                                    4 X 32 X 2

                                                                                         PROMPT MEMORY

15

15 X 34 LEADS

15 SELF

                                                                                         32K X 128 RAM

                   32 X 2
4 GHz SAMPLER

40

34

40 X 40 MATRIX OF CORRELATOR CHIPS

34 SELF

128 REQUIRED

15 X 34 LAGS

                                                                                                                     BASELINE ELECTRONICS
                                                                                        STATION ELECTRONICS

                                                  FIGURE 1